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Perth DC Mobile Plant Specifications and Operating Data Extract
Manufacturer specifications, operator manual extracts and the February 2026 plant movement count
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	Applies to
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	Status
	Controlled. Uncontrolled when printed



1. About this extract
This extract brings together the manufacturer information and operating data for the mobile plant listed in SRL-CR-066 Plant Register, Perth DC. Sections 2 to 4 are taken from the manufacturers' specification sheets and operator manuals held in Limble CMMS against each asset. Section 5 is the result of a one-week count of plant movements carried out by the WHS team. Make and model names in this extract are simulated.
1. Prepared by Maya Atherton, WHS Administration Officer, and Tariq Ahmed, Graduate WHS Officer, for the WHS Coordinator.
1. Speeds are the manufacturer's rated maximum travel speeds on a level, dry floor. They are not measured speeds at the Perth DC.
1. Site rules for operating the plant are in SRL-CR-042; traffic routes and zones are in SRL-CR-043.
2. Plant covered
	Asset ID
	Type
	Make and model
	Power
	Year
	Main work areas (SRL-CR-066)

	FL-01
	Counterbalance forklift, 2.5 t
	Arcmont AC25-G
	LPG (18 kg cylinder)
	2019
	Inbound docks 1 and 2, staging, yard

	FL-02
	Counterbalance forklift, 2.5 t
	Arcmont AC25-G
	LPG (18 kg cylinder)
	2020
	Inbound docks 3 and 4, dispatch lanes, yard

	FL-03
	Counterbalance forklift, 2.0 t
	Arcmont AC20-E
	Electric, 48 V lead-acid traction battery
	2021
	Pick zones A to C, refrigerated zone

	RT-01
	Reach truck
	Arcmont RX16
	Electric, 48 V lead-acid traction battery
	2022
	Racking rows 1 to 5; replenishment of pick faces in Zones A to C

	RT-02
	Reach truck
	Arcmont RX16
	Electric, 48 V lead-acid traction battery
	2022
	Racking rows 6 to 10; replenishment of pick faces in Zones A to C

	PJ-01, PJ-02
	Electric pallet jack (walk-behind)
	Braxa EP20
	Electric, 24 V battery
	2023
	Pick zone B, inbound staging, dispatch lanes

	WS-01
	Walkie stacker (walk-behind)
	Braxa WS12
	Electric, 24 V battery
	2022
	Inbound staging


3. Specification extract
	Specification
	AC25-G (FL-01, FL-02)
	AC20-E (FL-03)
	RX16 (RT-01, RT-02)
	EP20 (PJ-01, PJ-02)
	WS12 (WS-01)

	Rated capacity and load centre
	2,500 kg at 500 mm
	2,000 kg at 500 mm
	1,600 kg at 600 mm
	2,000 kg at 600 mm
	1,200 kg at 600 mm

	Maximum lift height
	4,500 mm
	4,500 mm
	9,500 mm
	200 mm (pallet lift only)
	3,300 mm

	Travel speed, unladen (maximum)
	19 km/h
	18 km/h
	12 km/h
	6 km/h
	5.5 km/h

	Travel speed, laden (maximum)
	18 km/h
	17 km/h
	11 km/h
	5 km/h
	5 km/h

	Service weight (without load)
	3,950 kg
	3,600 kg
	2,900 kg
	480 kg
	1,150 kg

	Operator position
	Seated, facing forward
	Seated, facing forward
	Seated sideways to the direction of travel
	Walking behind the tiller
	Walking behind the tiller

	Warning devices fitted as standard
	Horn; headlights; rear work light; amber rotating beacon (dash switch); reversing alarm
	Horn; headlights; rear work light; amber rotating beacon (dash switch); reversing alarm
	Horn; work lights; amber rotating beacon (dash switch); reversing alarm
	Horn
	Horn

	Operator protection
	Overhead guard; load backrest; seatbelt; seat switch
	Overhead guard; load backrest; seatbelt; seat switch
	Overhead guard; dead-man pedal
	Belly button reverse; brake on tiller release
	Belly button reverse; brake on tiller release

	Factory options available
	Speed limiting; blue pedestrian warning spotlight; beacon wired to the ignition
	Speed limiting; blue pedestrian warning spotlight; beacon wired to the ignition
	Speed limiting; blue pedestrian warning spotlight
	Not applicable
	Not applicable

	Options fitted at the Perth DC
	None
	None
	None
	Not applicable
	Not applicable


4. Operator manual extracts
The following extracts are taken from the operator manuals. Wording is summarised; the full manuals are in Limble CMMS.
	Topic
	Counterbalance forklifts (AC25-G, AC20-E)
	Reach trucks (RX16)

	Visibility with loads
	A carried load can block the operator's forward view. When the load blocks the forward view, travel in reverse, looking in the direction of travel, or use a spotter to guide you.
	Bulky loads and the mast restrict vision. When the load blocks the view in the direction of travel, travel in the other direction or use a spotter. Lower the load before travelling.

	Reversing
	Before reversing, look over both shoulders in the direction of travel. The reversing alarm warns people nearby but does not replace looking. Rear vision is restricted by the counterweight and the overhead guard posts.
	The operator sits sideways and must turn the head to see in either direction of travel. Check both directions before moving.

	Speed
	Travel at a speed that allows the truck to be stopped safely within the distance that can be seen to be clear. Reduce speed at corners, on wet or uneven floors and where people are present. Stopping distance increases with speed and load.
	Travel slowly in aisles and at aisle ends. Never travel with the mast extended or the load raised.

	Load handling
	Carry loads low with the mast tilted back. Do not lift or lower while travelling. Do not lift a load over any person.
	Do not raise or lower loads while people are below or next to the load. Extend the reach only when stationary.

	Rotating beacon
	The beacon is switched on and off by the operator at the dash switch. A factory option wires the beacon so that it operates whenever the truck is switched on.
	As for counterbalance forklifts.

	Speed limiting option
	An authorised service technician can set a maximum travel speed for the truck. The setting applies wherever the truck travels and is changed only by the technician.
	As for counterbalance forklifts.

	Daily checks
	Brakes, steering, horn, lights, beacon, reversing alarm, seatbelt and seat switch, forks, mast and chains, hydraulic leaks, tyres, LPG system (AC25-G) or battery (AC20-E).
	Brakes, steering, horn, lights, beacon, reversing alarm, dead-man pedal, reach mechanism, forks, mast and chains, hydraulic leaks, battery.


5. Plant movement count, February 2026
The WHS team counted forklift and reach truck movements at the Perth DC for one week, from Monday 16 to Sunday 22 February 2026, using observers at fixed points on each shift. A movement is one trip by a forklift or reach truck from one location to another (for example dock to staging, staging to racking, or racking to a pick face). Pallet jack and walkie stacker trips were not counted.
5.1 Average movements per hour by shift
	Shift
	Hours
	Average forklift and reach truck movements per hour
	Peak period
	Average movements per hour in the peak period
	Counterbalance forklift share (average per hour)
	Reach truck share (average per hour)

	Morning
	06:00 to 14:00, Monday to Friday
	46
	06:00 to 09:00 (inbound container peak)
	71
	38
	8

	Afternoon
	14:00 to 22:00, Monday to Friday
	39
	14:00 to 16:30 (dispatch and line haul loading peak)
	63
	33
	6

	Overnight
	22:00 to 06:00, Sunday night to Friday morning
	22
	None recorded
	
	7
	15

	Weekend
	07:00 to 17:00, Saturday and Sunday
	18
	None recorded
	
	14
	4


5.2 Other observations recorded during the count
	Observation
	Detail

	Pedestrians at the 14:00 shift changeover
	About 40 people moving to and from the meal room through dispatch and Zone C between about 13:50 and 14:15.

	Reach truck replenishment of pick faces
	Mostly between 22:00 and 02:00 on the overnight shift, in the pick aisles of Zones A to C.

	Inbound peak
	Container and truck unloading at docks 1 to 4 between 06:00 and 09:00, with pallets staged in inbound staging before putaway.

	Dispatch peak
	Line haul and delivery loading at outbound docks 5 to 12 between 14:00 and 16:30.


6. Related documents
1. SRL-CR-042 Mobile Plant (Forklift and MHE) Operations Safe Operating Procedure
1. SRL-CR-043 Traffic Management Procedure and Plan, Perth DC
1. SRL-CR-049 Plant Pre-start Check Procedure; SRL-CR-075 Forklift and MHE Pre-start Checklist
1. SRL-CR-066 Plant Register, Perth DC
Document history
	Version
	Date
	Summary of change
	Approved by

	1.0
	27 February 2026
	First issue: specification and manual extracts for the Perth DC mobile plant and the results of the one-week movement count (16 to 22 February 2026).
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