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Dangerous Goods Manifest, Perth DC
Dangerous goods and combustible liquids stored at the Perth DC, for emergency services
	Document number
	SRL-CR-067
	Version
	3.0

	Document owner
	Daniela Marquez, WHS Coordinator (candidate role in some units), manifest holder
	Effective date
	2 March 2026

	Approved by
	Priya Sharma, National WHS Manager (Dangerous Goods Officer)
	Next review
	March 2027, or within 5 working days of any change

	Applies to
	Perth DC, Lot 14 Kewdale Road, Kewdale WA 6105
	Status
	Controlled. Uncontrolled when printed



	For emergency services
Site emergency controller in business hours: Distribution Centre Manager. After hours: the supervisor on duty. Meet at gate 1.
The site plan showing the storage areas, exits, hydrants and emergency equipment is kept with this manifest (SRL-CR-004 Perth DC Site Profile and Site Plan).


1. Manifest details
	Item
	Detail

	Site name and address
	SteelRiver Logistics Perth DC, Lot 14 Kewdale Road, Kewdale WA 6105

	Occupier
	SteelRiver Logistics Pty Ltd (ABN 59 412 088 731)

	Law
	Dangerous Goods Safety Act 2004 (WA) and Dangerous Goods Safety (Storage and Handling of Non-explosives) Regulations 2007 (WA); hazardous chemicals duties in the Work Health and Safety (General) Regulations 2022 (WA)

	Site classification
	Storage of dangerous goods below the Major Hazard Facility thresholds

	Manifest holder
	WHS Coordinator, Perth DC, supported by the Operations Manager

	Dangerous Goods Officer
	Priya Sharma, National WHS Manager

	Date prepared
	2 March 2026

	Next review
	March 2027, or within 5 working days of any change

	Where the manifest is kept
	Manifest box at gate 1 (main gate, Kewdale Road), weatherproof, with a "Hazchem Manifest" sign. A second copy is in the WHS office.

	Manifest box key
	Admin building reception

	Site plan
	SRL-CR-004 Perth DC Site Profile and Site Plan, kept in the manifest box with this manifest

	Emergency response
	The DC Manager (Lisa Anand, candidate role in some units) is the site emergency controller. DFES is the primary emergency agency. Emergency arrangements: SRL-CR-014 Emergency Management Plan, Perth DC, and SRL-CR-036 Emergency Response and Evacuation Procedures, Perth DC.


2. Storage areas
	Storage area
	Location
	Classes stored
	Maximum quantity
	Emergency equipment
	Key controls

	DG-AREA-01
	Yard, north-east corner: bulk diesel tank
	C1 combustible liquid
	5,000 L diesel
	Extinguishers EX-28 and EX-29 (dry chemical 9 kg); emergency stop on the pump; diesel spill kit SK-01 (kept inside inbound dock 1)
	Bunded steel tank; no smoking or ignition sources; delivery supervised by the inbound lead

	DG-AREA-02
	Indoor: battery charging bay, west wall north of inbound dock 4
	Class 8
	200 L battery electrolyte (in service)
	Eyewash and shower ES-01; acid spill kit SK-02 (neutraliser); extinguisher EX-12 (CO2 3.5 kg); charger isolator outside the bay door
	Bunded concrete floor; extraction fan; chargers on a separate isolator

	DG-AREA-03
	Outdoor gas cage, east boundary near gate 2
	Class 2.1 and Class 2.2
	1 acetylene and 1 oxygen cylinder (G size); up to 6 LPG cylinders of 18 kg
	Extinguisher EX-30 (dry chemical 9 kg)
	Open-air mesh cage; cylinders chained upright; flammable and oxidising gases separated; no ignition sources

	DG-AREA-04
	Indoor: cleaning store, locked, near the amenities
	Class 8 and Class 2.1
	100 L Class 8 liquids; 12 aerosol cans
	Extinguisher EX-25 (dry chemical 4.5 kg); eyewash station ES-02; general spill kit SK-03
	Lockable store; bunded shelving; hypochlorite kept apart from acids; flammable goods cabinet for aerosols


3. Substances
	No.
	Proper shipping name
	UN number
	Class or division
	Packing group
	Maximum quantity
	Container
	Storage area
	Hazchem code

	1
	Diesel fuel
	UN 1202
	C1 combustible liquid (not Class 3)
	III
	5,000 L
	Bulk steel tank, bunded
	DG-AREA-01
	Not required (C1)

	2
	Battery fluid, acid (sulfuric acid electrolyte)
	UN 2796
	Class 8
	II
	200 L (in service)
	In lead-acid traction batteries
	DG-AREA-02
	2R

	3
	Caustic alkali liquid, n.o.s. (industrial degreaser)
	UN 1719
	Class 8
	II
	60 L
	20 L drums
	DG-AREA-04
	2R

	4
	Hypochlorite solution (sodium hypochlorite 12.5%)
	UN 1791
	Class 8
	III
	40 L
	20 L drums
	DG-AREA-04
	2X

	5
	Aerosols, flammable (lubricant)
	UN 1950
	Class 2.1
	Not applicable
	12 cans (4.8 L)
	Aerosol cans in a flammable goods cabinet
	DG-AREA-04
	2YE

	6
	Acetylene, dissolved
	UN 1001
	Class 2.1
	Not applicable
	1 cylinder (G size)
	Pressure cylinder
	DG-AREA-03
	2SE

	7
	Oxygen, compressed
	UN 1072
	Class 2.2 (subsidiary 5.1)
	Not applicable
	1 cylinder (G size)
	Pressure cylinder
	DG-AREA-03
	2S

	8
	Liquefied petroleum gas (forklift fuel)
	UN 1075
	Class 2.1
	Not applicable
	Up to 6 x 18 kg (2 fitted to forklifts FL-01 and FL-02)
	Forklift gas cylinders
	DG-AREA-03
	2YE


4. Emergency contacts
	Contact
	Number

	Fire, ambulance, police
	000

	DFES (emergency information line)
	13 33 37

	Alarm monitoring company (24 hours)
	1300 975 708

	WorkSafe WA (work health and safety and dangerous goods safety)
	1300 307 877

	Dangerous Goods Officer: Priya Sharma, National WHS Manager
	Mobile on the emergency contacts sheet in the manifest box

	Site emergency controller: DC Manager
	Mobile on the emergency contacts sheet in the manifest box

	After hours: supervisor on duty
	Gatehouse phone and the duty supervisor mobile on the emergency contacts sheet


5. Keeping the manifest current
1. The manifest holder updates the manifest within 5 working days of any change to the dangerous goods on site: a new substance, a substance removed, or a change to a maximum quantity or storage area. SRL-CR-065 Hazardous Chemicals Register, Perth DC, is updated at the same time.
1. The manifest is reviewed at least once a year and after any change to the site layout.
1. A copy of the manifest and site plan is given to DFES on request and at any DFES site familiarisation visit.
1. Any dangerous goods incident (a spill, leak, fire or release involving dangerous goods) is reported at once to the site emergency controller and the Dangerous Goods Officer, who decides whether the regulator must be notified.
Document history
	Version
	Date
	Summary of change
	Approved by

	3.0
	2 March 2026
	Annual review. Renumbered SRL-CR-067. Dangerous Goods Officer changed to the National WHS Manager. LPG forklift cylinders listed in DG-AREA-03. Diesel shown as a C1 combustible liquid. Regulator contact updated to WorkSafe WA. Site plan reference changed to SRL-CR-004.
	Priya Sharma, National WHS Manager
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